|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Manufacturer** | **Part Number** | **Description** | **Qty** | **Ordering Website** |
| TE Connectivity AMP | 5787394-2 | 26 Position D-Type Receptacle, Female Sockets Connector, Board Edge, Through Hole, Right Angle Solder | 1 | https://www.digikey.com/product-detail/en/te-connectivity-amp-connectors/5787394-2/A35093-ND/1279806 |
| Grayhill Inc. | 51P22-01-1-16N | Rotary Switch 16 Position SP16T 150mA (AC), 200mA (DC) 115VAC Panel Mount, Through Hole | 1 | https://www.digikey.com/product-detail/en/grayhill-inc/51P22-01-1-16N/GH7687-ND/418013 |
| Grayhill Inc. | 11K5028-JMNB | KNOB CONTROL NYLON .125" BLK | 1 | https://www.digikey.com/product-detail/en/grayhill-inc/11K5028-JMNB/GH7662-ND/1860233 |
| Sparkfun | PRT-12807 | Header - 2x3 (Male, 0.1") | 2 | https://www.sparkfun.com/products/12807 |
| Sparkfun | PRT-00116 | Break Away Headers – Straight, 40 pins 0.1” | 1 | https://www.sparkfun.com/products/116 |
| Sparkfun | PRT-09044 | Jumper - 2 Pin, shunts, 0.1” | 2 | https://www.sparkfun.com/products/9044 |
|  |  |  |  |  |